DE2_SOPC |

2012.02.03.11:05:16 | Datasheet

Overview

clk_50 | DE2_SOPC
| led
| out_port

Processor
cpu Nios II 11.1
All Components
cpu altera_nios2 11.1
sysid altera_avalon_sysid 11.1
jtag_uart altera_avalon_jtag_uart 11.1
onchip_memory2 altera_avalon_onchip_memory2 11.1
led altera_avalon_pio 11.1
Memory Map

| cpu
instruction_master | data_master
cpu |  |
jtag_debug_module | 0x00020800 | 0x00020800
sysid |  |
control_slave |  | 0x00021010
jtag_uart |  |
avalon_jtag_slave |  | 0x00021018
onchip_memory2 |  |
s1 | 0x00010000 | 0x00010000
led |  |
s1 |  | 0x00021000

## clk_50

clock_source v11.1

## Parameters
clockFrequency | 50000000
clockFrequencyKnown | true
inputClockFrequency | 0
resetSynchronousEdges | NONE
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## cpu

altera_nios2 v11.1

clk_50 | clk | cpu
clk
|  | data_master | sysid
|  | control_slave
|  | data_master | jtag_uart
|  | avalon_jtag_slave
|  | d_irq
|  | irq
|  | instruction_master | onchip_memory2
|  | s1
|  | data_master
|  | s1
|  | data_master | led
|  | s1

## Parameters
userDefinedSettings |
tightlyCoupledInstructionMaster3MapParam |
tightlyCoupledInstructionMaster3AddrWidth | 1
tightlyCoupledInstructionMaster2MapParam |
tightlyCoupledInstructionMaster2AddrWidth | 1
tightlyCoupledInstructionMaster1MapParam |
tightlyCoupledInstructionMaster1AddrWidth | 1
tightlyCoupledInstructionMaster0MapParam |
tightlyCoupledInstructionMaster0AddrWidth | 1
tightlyCoupledDataMaster3MapParam |
tightlyCoupledDataMaster3AddrWidth | 1
tightlyCoupledDataMaster2MapParam |
tightlyCoupledDataMaster2AddrWidth | 1
tightlyCoupledDataMaster1MapParam |
tightlyCoupledDataMaster1AddrWidth | 1
tightlyCoupledDataMaster0MapParam |
tightlyCoupledDataMaster0AddrWidth | 1
setting_showUnpublishedSettings | false
setting_showInternalSettings | false
setting_shadowRegisterSets | 0
setting_preciseSlaveAccessErrorException | false
setting_preciseIllegalMemAccessException | false
setting_preciseDivisionErrorException | false
setting_performanceCounter | false
setting_perfCounterWidth | _32
setting_interruptControllerType | Internal
setting_illegalMemAccessDetection | false
setting_illegalInstructionsTrap | false
setting_fullWaveformSignals | false
setting_extraExceptionInfo | false
setting_exportPCB | false
setting_debugSimGen | false
setting_clearXBitsLDNonBypass | true
setting_branchPredictionType | Automatic
setting_bit31BypassDCache | true
setting_bigEndian | false
setting_bhtPtrSz | _8
setting_bhtIndexPcOnly | false
setting_avalonDebugPortPresent | false
setting_alwaysEncrypt | true
setting_allowFullAddressRange | false
setting_activateTrace | true
setting_activateTestEndChecker | false
setting_activateMonitors | true
setting_activateModelChecker | false
setting_HDLSimCachesCleared | true
setting_HBreakTest | false
resetSlave | onchip_memory2.s1
resetOffset | 0
muldiv_multiplierType | EmbeddedMulFast
muldiv_divider | false
mpu_useLimit | false
mpu_numOfInstRegion | 8
mpu_numOfDataRegion | 8
mpu_minInstRegionSize | _12
mpu_minDataRegionSize | _12
mpu_enabled | false
mmu_uitlbNumEntries | _4
mmu_udtlbNumEntries | _6
mmu_tlbPtrSz | _7
mmu_tlbNumWays | _16
mmu_processIDNumBits | _8
mmu_enabled | false
mmu_autoAssignTlbPtrSz | true
mmu_TLBMissExcSlave |
mmu_TLBMissExcOffset | 0
manuallyAssignCpuID | false
internalIrqMaskSystemInfo | 1
instSlaveMapParam | <address-map><slave name='onchip_memory2.s1' start='0x10000' end='0x1A000' /><slave name='cpu.jtag_debug_module' start='0x20800' end='0x21000' /></address-map>
instAddrWidth | 18
impl | Fast
icache_size | _4096
icache_ramBlockType | Automatic
icache_numTCIM | _0
icache_burstType | None
exceptionSlave | onchip_memory2.s1
exceptionOffset | 32
deviceFeaturesSystemInfo | ADDRESS_STALL 1 CELL_LEVEL_BACK_ANNOTATION_DISABLED 0 COMPILER_SUPPORT 1 DSP 0 DSP_SHIFTER_BLOCK 0 DUMP_ASM_LAB_BITS_FOR_POWER 1 EMUL 1 ENABLE_ADVANCED_IO_ANALYSIS_GUI_FEATURES 0 EPCS 1 ESB 0 FAKE1 0 FAKE2 0 FAKE3 0 FITTER_USE_FALLING_EDGE_DELAY 0 GENERATE_DC_ON_CURRENT_WARNING_FOR_INTERNAL_CLAMPING_DIODE 0 HARDCOPY 0 HAS_18_BIT_MULTS 0 HAS_ACE_SUPPORT 1 HAS_ADJUSTABLE_OUTPUT_IO_TIMING_MEAS_POINT 0 HAS_ADVANCED_IO_INVERTED_CORNER 0 HAS_ADVANCED_IO_POWER_SUPPORT 0 HAS_ADVANCED_IO_TIMING_SUPPORT 0 HAS_ALM_SUPPORT 0 HAS_ATOM_AND_ROUTING_POWER_MODELED_TOGETHER 0 HAS_AUTO_DERIVE_CLOCK_UNCERTAINTY_SUPPORT 0 HAS_AUTO_FIT_SUPPORT 1 HAS_BALANCED_OPT_TECHNIQUE_SUPPORT 1 HAS_BENEFICIAL_SKEW_SUPPORT 0 HAS_BITLEVEL_DRIVE_STRENGTH_CONTROL 0 HAS_BSDL_FILE_GENERATION 0 HAS_CGA_SUPPORT 1 HAS_CHECK_NETLIST_SUPPORT 1 HAS_CLOCK_REGION_CHECKER_ENABLED 1 HAS_CORE_JUNCTION_TEMP_DERATING 1 HAS_CROSSTALK_SUPPORT 0 HAS_CUSTOM_REGION_SUPPORT 1 HAS_DATA_DRIVEN_ACVQ_HSSI_SUPPORT 0 HAS_DDB_FDI_SUPPORT 0 HAS_DESIGN_ANALYZER_SUPPORT 1 HAS_DETAILED_IO_RAIL_POWER_MODEL 1 HAS_DETAILED_LEIM_STATIC_POWER_MODEL 0 HAS_DETAILED_LE_POWER_MODEL 1 HAS_DETAILED_ROUTING_MUX_STATIC_POWER_MODEL 0 HAS_DETAILED_THERMAL_CIRCUIT_PARAMETER_SUPPORT 1 HAS_DEVICE_MIGRATION_SUPPORT 1 HAS_DIAGONAL_MIGRATION_SUPPORT 0 HAS_EMIF_TOOLKIT_SUPPORT 0 HAS_FAMILY_VARIANT_MIGRATION_SUPPORT 0 HAS_FANOUT_FREE_NODE_SUPPORT 1 HAS_FAST_FIT_SUPPORT 1 HAS_FITTER_EARLY_TIMING_ESTIMATE_SUPPORT 1 HAS_FITTER_ECO_SUPPORT 1 HAS_FIT_NETLIST_OPT_RETIME_SUPPORT 1 HAS_FIT_NETLIST_OPT_SUPPORT 1 HAS_FORMAL_VERIFICATION_SUPPORT 1 HAS_FPGA_XCHANGE_SUPPORT 1 HAS_FSAC_LUTRAM_REGISTER_PACKING_SUPPORT 0 HAS_FULL_DAT_MIN_TIMING_SUPPORT 1 HAS_FULL_INCREMENTAL_DESIGN_SUPPORT 1 HAS_FUNCTIONAL_SIMULATION_SUPPORT 1 HAS_GLITCH_FILTERING_SUPPORT 1 HAS_HC_READY_SUPPORT 0 HAS_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_HOLD_TIME_AVOIDANCE_ACROSS_CLOCK_SPINE_SUPPORT 1 HAS_HSPICE_WRITER_SUPPORT 0 HAS_HSSI_POWER_CALCULATOR 0 HAS_IBISO_WRITER_SUPPORT 1 HAS_INCREMENTAL_DAT_SUPPORT 0 HAS_INCREMENTAL_SYNTHESIS_SUPPORT 1 HAS_IO_ASSIGNMENT_ANALYSIS_SUPPORT 1 HAS_IO_DECODER 0 HAS_IO_PLACEMENT_OPTIMIZATION_SUPPORT 1 HAS_IO_SMART_RECOMPILE_SUPPORT 1 HAS_JITTER_SUPPORT 0 HAS_JTAG_SLD_HUB_SUPPORT 1 HAS_LOGIC_LOCK_SUPPORT 1 HAS_MICROPROCESSOR 0 HAS_MIF_SMART_COMPILE_SUPPORT 1 HAS_MINMAX_TIMING_MODELING_SUPPORT 0 HAS_MIN_TIMING_ANALYSIS_SUPPORT 1 HAS_MUX_RESTRUCTURE_SUPPORT 1 HAS_NEW_HC_FLOW_SUPPORT 0 HAS_NEW_SERDES_MAX_RESOURCE_COUNT_REPORTING_SUPPORT 0 HAS_NEW_VPR_SUPPORT 1 HAS_NONSOCKET_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_NO_JTAG_USERCODE_SUPPORT 0 HAS_OPERATING_SETTINGS_AND_CONDITIONS_REPORTING_SUPPORT 1 HAS_PAD_LOCATION_ASSIGNMENT_SUPPORT 1 HAS_PARTIAL_RECONFIG_SUPPORT 0 HAS_PHYSICAL_NETLIST_OUTPUT 0 HAS_PHYSICAL_ROUTING_SUPPORT 0 HAS_PIN_SPECIFIC_VOLTAGE_SUPPORT 0 HAS_PLDM_REF_SUPPORT 1 HAS_POWER_ESTIMATION_SUPPORT 1 HAS_PRELIMINARY_CLOCK_UNCERTAINTY_NUMBERS 0 HAS_PRE_FITTER_FPP_SUPPORT 0 HAS_PRE_FITTER_LUTRAM_NETLIST_CHECKER_ENABLED 0 HAS_PVA_SUPPORT 1 HAS_RCF_SUPPORT 1 HAS_RCF_SUPPORT_FOR_DEBUGGING 0 HAS_RED_BLACK_SEPARATION_SUPPORT 0 HAS_RE_LEVEL_TIMING_GRAPH_SUPPORT 0 HAS_RISEFALL_DELAY_SUPPORT 1 HAS_SIGNAL_PROBE_SUPPORT 1 HAS_SIGNAL_TAP_SUPPORT 1 HAS_SIMULATOR_SUPPORT 1 HAS_SPLIT_IO_SUPPORT 0 HAS_SPLIT_LC_SUPPORT 1 HAS_SYNTH_FSYN_NETLIST_OPT_SUPPORT 0 HAS_SYNTH_NETLIST_OPT_RETIME_SUPPORT 1 HAS_SYNTH_NETLIST_OPT_SUPPORT 1 HAS_TECHNOLOGY_MIGRATION_SUPPORT 0 HAS_TEMPLATED_REGISTER_PACKING_SUPPORT 1 HAS_TIME_BORROWING_SUPPORT 0 HAS_TIMING_DRIVEN_SYNTHESIS_SUPPORT 1 HAS_TIMING_INFO_SUPPORT 1 HAS_TIMING_OPERATING_CONDITIONS 0 HAS_TIMING_SIMULATION_SUPPORT 1 HAS_TITAN_BASED_MAC_REGISTER_PACKER_SUPPORT 0 HAS_USER_HIGH_SPEED_LOW_POWER_TILE_SUPPORT 0 HAS_USE_FITTER_INFO_SUPPORT 1 HAS_VCCPD_POWER_RAIL 0 HAS_VERTICAL_MIGRATION_SUPPORT 1 HAS_VIEWDRAW_SYMBOL_SUPPORT 1 HAS_VIO_SUPPORT 1 HAS_VIRTUAL_DEVICES 0 HAS_WYSIWYG_DFFEAS_SUPPORT 0 HAS_XIBISO_WRITER_SUPPORT 0 INCREMENTAL_DESIGN_SUPPORTS_COMPATIBLE_CONSTRAINTS 0 INSTALLED 0 IS_CONFIG_ROM 0 IS_DEFAULT_FAMILY 0 IS_HARDCOPY_FAMILY 0 LVDS_IO 0 M10K_MEMORY 0 M144K_MEMORY 0 M20K_MEMORY 0 M4K_MEMORY 1 M512_MEMORY 0 M9K_MEMORY 0 MLAB_MEMORY 0 MRAM_MEMORY 0 NOT_LISTED 0 NO_RPE_SUPPORT 0 NO_SUPPORT_FOR_LOGICLOCK_CONTENT_BACK_ANNOTATION 0 NO_SUPPORT_FOR_STA_CLOCK_UNCERTAINTY_CHECK 1 NO_TDC_SUPPORT 0 POSTFIT_BAK_DATABASE_EXPORT_ENABLED 1 POSTMAP_BAK_DATABASE_EXPORT_ENABLED 1 PROGRAMMER_SUPPORT 1 QFIT_IN_DEVELOPMENT 0 QMAP_IN_DEVELOPMENT 0 RAM_LOGICAL_NAME_CHECKING_IN_CUT_ENABLED 1 REPORTS_METASTABILITY_MTBF 0 REQUIRES_INSTALLATION_PATCH 0 REQUIRES_LIST_OF_TEMPERATURE_AND_VOLTAGE_OPERATING_CONDITIONS 0 RESERVES_SIGNAL_PROBE_PINS 0 RESOLVE_MAX_FANOUT_EARLY 1 RESOLVE_MAX_FANOUT_LATE 0 RESPECTS_FIXED_SIZED_LOCKED_LOCATION_LOGICLOCK 1 RESTRICTED_USER_SELECTION 0 RISEFALL_SUPPORT_IS_HIDDEN 1 SUPPORTS_ADDITIONAL_OPTIONS_FOR_UNUSED_IO 1 SUPPORTS_CRC 1 SUPPORTS_DIFFERENTIAL_AIOT_BOARD_TRACE_MODEL 0 SUPPORTS_DSP_BALANCING_BACK_ANNOTATION 0 SUPPORTS_GENERATION_OF_EARLY_POWER_ESTIMATOR_FILE 1 SUPPORTS_GLOBAL_SIGNAL_BACK_ANNOTATION 0 SUPPORTS_MAC_CHAIN_OUT_ADDER 0 SUPPORTS_RAM_PACKING_BACK_ANNOTATION 0 SUPPORTS_REG_PACKING_BACK_ANNOTATION 0 SUPPORTS_SIGNALPROBE_REGISTER_PIPELINING 1 SUPPORTS_SINGLE_ENDED_AIOT_BOARD_TRACE_MODEL 0 SUPPORTS_USER_MANUAL_LOGIC_DUPLICATION 1 TMV_RUN_CUSTOMIZABLE_VIEWER 1 TMV_RUN_INTERNAL_DETAILS 1 TMV_RUN_INTERNAL_DETAILS_ON_IO 1 TMV_RUN_INTERNAL_DETAILS_ON_IOBUF 0 TMV_RUN_INTERNAL_DETAILS_ON_LCELL 0 TMV_RUN_INTERNAL_DETAILS_ON_LRAM 0 TRANSCEIVER_3G_BLOCK 0 TRANSCEIVER_6G_BLOCK 0 USES_ACV_FOR_FLED 1 USES_ADB_FOR_BACK_ANNOTATION 0 USES_ASIC_ROUTING_POWER_CALCULATOR 0 USES_DATA_DRIVEN_PLL_COMPUTATION_UTIL 1 USES_DEV 1 USES_ICP_FOR_ECO_FITTER 0 USES_LIBERTY_TIMING 0 USES_POWER_SIGNAL_ACTIVITIES 1 USES_THIRD_GENERATION_TIMING_MODELS_TIS 0 USE_ADVANCED_IO_POWER_BY_DEFAULT 0 USE_ADVANCED_IO_TIMING_BY_DEFAULT 0 USE_BASE_FAMILY_DDB_PATH 0 USE_OCT_AUTO_CALIBRATION 0 USE_RISEFALL_ONLY 0 USE_SEPARATE_LIST_FOR_TECH_MIGRATION 0 USE_SINGLE_COMPILER_PASS_PLL_MIF_FILE_WRITER 0 USE_TITAN_IO_BASED_IO_REGISTER_PACKER_UTIL 0 WYSIWYG_BUS_WIDTH_CHECKING_IN_CUT_ENABLED 0
deviceFamilyName | Cyclone II
debug_triggerArming | true
debug_level | Level1
debug_jtagInstanceID | 0
debug_embeddedPLL | true
debug_debugReqSignals | false
debug_assignJtagInstanceID | false
debug_OCIOnchipTrace | _128
dcache_size | _2048
dcache_ramBlockType | Automatic
dcache_omitDataMaster | false
dcache_numTCDM | _0
dcache_lineSize | _32
dcache_bursts | false
dataSlaveMapParam | <address-map><slave name='onchip_memory2.s1' start='0x10000' end='0x1A000' /><slave name='cpu.jtag_debug_module' start='0x20800' end='0x21000' /><slave name='led.s1' start='0x21000' end='0x21010' /><slave name='sysid.control_slave' start='0x21010' end='0x21018' /><slave name='jtag_uart.avalon_jtag_slave' start='0x21018' end='0x21020' /></address-map>
dataAddrWidth | 18
customInstSlavesSystemInfo | <info/>
cpuReset | false
cpuID | 0
clockFrequency | 50000000
breakSlave | cpu.jtag_debug_module
breakOffset | 32
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
CPU_IMPLEMENTATION | "fast"
BIG_ENDIAN | 0
CPU_FREQ | 50000000u
ICACHE_LINE_SIZE | 32
ICACHE_LINE_SIZE_LOG2 | 5
ICACHE_SIZE | 4096
DCACHE_LINE_SIZE | 32
DCACHE_LINE_SIZE_LOG2 | 5
DCACHE_SIZE | 2048
INITDA_SUPPORTED |
FLUSHDA_SUPPORTED |
HAS_JMPI_INSTRUCTION |
EXCEPTION_ADDR | 0x10020
RESET_ADDR | 0x10000
BREAK_ADDR | 0x20820
HAS_DEBUG_STUB |
HAS_DEBUG_CORE | 1
CPU_ID_SIZE | 1
CPU_ID_VALUE | 0x0
HARDWARE_DIVIDE_PRESENT | 0
HARDWARE_MULTIPLY_PRESENT | 1
HARDWARE_MULX_PRESENT | 0
INST_ADDR_WIDTH | 18
DATA_ADDR_WIDTH | 18
NUM_OF_SHADOW_REG_SETS | 0

## sysid

altera_avalon_sysid v11.1

clk_50 | clk | sysid
clk
cpu | data_master
control_slave

## Parameters
id | 0
timestamp | 1328238288
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
ID | 0u
TIMESTAMP | 1328238288u

## jtag_uart

altera_avalon_jtag_uart v11.1

clk_50 | clk | jtag_uart
clk
cpu | data_master
avalon_jtag_slave
d_irq
irq

## Parameters
allowMultipleConnections | false
hubInstanceID | 0
readBufferDepth | 64
readIRQThreshold | 8
simInputCharacterStream |
simInteractiveOptions | INTERACTIVE_ASCII_OUTPUT
useRegistersForReadBuffer | false
useRegistersForWriteBuffer | false
useRelativePathForSimFile | false
writeBufferDepth | 64
writeIRQThreshold | 8
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
WRITE_DEPTH | 64
READ_DEPTH | 64
WRITE_THRESHOLD | 8
READ_THRESHOLD | 8

## onchip_memory2

altera_avalon_onchip_memory2 v11.1

clk_50 | clk | onchip_memory2
clk1
cpu | instruction_master
s1
data_master
s1

## Parameters
allowInSystemMemoryContentEditor | false
autoInitializationFileName | onchip_memory2
blockType | AUTO
dataWidth | 32
deviceFamily | Cyclone II
dualPort | false
initMemContent | true
initializationFileName | onchip_memory2
instanceID | NONE
memorySize | 40960
readDuringWriteMode | DONT_CARE
simAllowMRAMContentsFile | false
simMemInitOnlyFilename | 0
singleClockOperation | false
slave1Latency | 1
slave2Latency | 1
useNonDefaultInitFile | false
useShallowMemBlocks | false
writable | true
generateLegacySim | false

## Software Assignments
ALLOW_MRAM_SIM_CONTENTS_ONLY_FILE | 0
INIT_CONTENTS_FILE | "onchip_memory2"
NON_DEFAULT_INIT_FILE_ENABLED | 0
GUI_RAM_BLOCK_TYPE | "Automatic"
WRITABLE | 1
DUAL_PORT | 0
SINGLE_CLOCK_OP | 0
SIZE_VALUE | 40960u
SIZE_MULTIPLE | 1
CONTENTS_INFO | ""
RAM_BLOCK_TYPE | "Auto"
INIT_MEM_CONTENT | 1
ALLOW_IN_SYSTEM_MEMORY_CONTENT_EDITOR | 0
INSTANCE_ID | "NONE"
READ_DURING_WRITE_MODE | "DONT_CARE"

## led

altera_avalon_pio v11.1

clk_50 | clk | led
clk
cpu | data_master
s1

## Parameters
bitClearingEdgeCapReg | false
bitModifyingOutReg | false
captureEdge | false
clockRate | 50000000
direction | Output
edgeType | RISING
generateIRQ | false
irqType | LEVEL
resetValue | 0
simDoTestBenchWiring | false
simDrivenValue | 0
width | 1
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments
DO_TEST_BENCH_WIRING | 0
DRIVEN_SIM_VALUE | 0x0
HAS_TRI | 0
HAS_OUT | 1
HAS_IN | 0
CAPTURE | 0
BIT_CLEARING_EDGE_REGISTER | 0
BIT_MODIFYING_OUTPUT_REGISTER | 0
DATA_WIDTH | 1
RESET_VALUE | 0x0
EDGE_TYPE | "NONE"
IRQ_TYPE | "NONE"
FREQ | 50000000u

generation took 0.02 seconds | rendering took 0.09 seconds