Altera SOPC Builder Version 5.10 Build 176
Copyright (c) 1999-2005 Altera Corporation.  All rights reserved.


# 2005.11.17 16:18:39 (*) mk_custom_sdk starting
# 2005.11.17 16:18:39 (*) Reading project C:/DE2/DE2_Board/system/DE2_Board.ptf.

# 2005.11.17 16:18:40 (*) Finding all CPUs

# 2005.11.17 16:18:40 (*) Finding all available components

# 2005.11.17 16:18:40 (*) Reading C:/DE2/DE2_Board/system/.sopc_builder/install.ptf

# 2005.11.17 16:18:40 (*) Found 52 components

# 2005.11.17 16:18:41 (*) Finding all peripherals

# 2005.11.17 16:18:41 (*) Finding software components

# 2005.11.17 16:18:42 (*) (Legacy SDK Generation Skipped)
# 2005.11.17 16:18:42 (*) (All TCL Script Generation Skipped)
# 2005.11.17 16:18:42 (*) (No Libraries Built)
# 2005.11.17 16:18:42 (*) (Contents Generation Skipped)
# 2005.11.17 16:18:42 (*) mk_custom_sdk finishing

# 2005.11.17 16:18:42 (*) Starting generation for system: DE2_Board.

.
..
.
.
.
.
.
.

# 2005.11.17 16:18:44 (*) Running Generator Program for cpu_0

# 2005.11.17 16:18:48 (*)   Checking for plaintext license.
# 2005.11.17 16:18:52 (*)   Plaintext license not found.
# 2005.11.17 16:18:52 (*)   Checking for encrypted license (non-evaluation).
# 2005.11.17 16:18:52 (*)   Encrypted license found.  SOF will not be time-limited.
# 2005.11.17 16:18:59 (*)   Creating encrypted HDL

# 2005.11.17 16:19:01 (*) Running Generator Program for firmware_ROM

# 2005.11.17 16:19:03 (*) Running Generator Program for data_RAM

# 2005.11.17 16:19:06 (*) Running Generator Program for payload_buffer

# 2005.11.17 16:19:08 (*) Running Generator Program for jtag_uart_0

# 2005.11.17 16:19:11 (*) Running Generator Program for sysid

# 2005.11.17 16:19:13 (*) Running Generator Program for asmi

# 2005.11.17 16:19:16 (*) Running Generator Program for Board_System

# 2005.11.17 16:19:17 (*) Now generating custom board component and flash programmer design.
# 2005.11.17 16:19:17 (*) After generation is complete, you must do the following next steps:
# 2005.11.17 16:19:17 (*)  1.) Update the system symbol in QuartusII
# 2005.11.17 16:19:17 (*)  2.) Add flash pins to the .bdf schematic file and connect them to the flash
# 2005.11.17 16:19:17 (*)       ports on the updated symbol.
# 2005.11.17 16:19:17 (*)  3.) Add pins to the .bdf schematic file to dissable any other external devices

# 2005.11.17 16:19:17 (*)       that are on the same tri-state bus as flash.
# 2005.11.17 16:19:17 (*)   4.) Assign the schematic pins you added to the associated device pins that
# 2005.11.17 16:19:17 (*)       connect to the external devices
# 2005.11.17 16:19:17 (*)  5.) Compile the design in QuartusII.
# 2005.11.17 16:19:17 (*) It is important that you consult the document "NiosII Flash Programmer User Guide",
# 2005.11.17 16:19:17 (*)  available at www.altera.com, before attempting to port the NiosII Flash Programmer

# 2005.11.17 16:19:17 (*)  to custom boards.


# 2005.11.17 16:19:18 (*) Running Generator Program for cfi_flash_0


# 2005.11.17 16:19:19 (*) Making arbitration and system (top) modules.

# 2005.11.17 16:19:27 (*) Generating Quartus symbol for top level: DE2_Board

# 2005.11.17 16:19:27 (*) Generating Symbol C:/DE2/DE2_Board/system/DE2_Board.bsf

# 2005.11.17 16:19:27 (*) Creating command-line system-generation script: C:/DE2/DE2_Board/system/DE2_Board_generation_script

# 2005.11.17 16:19:27 (*) Running setup for HDL simulator: modelsim


# 2005.11.17 16:19:27 (*) Setting up Quartus with DE2_Board_setup_quartus.tcl
c:/altera/quartus51/bin/quartus_sh -t DE2_Board_setup_quartus.tcl


Info: *******************************************************************
Info: Running Quartus II Shell
    Info: Version 5.1 Build 176 10/26/2005 SJ Full Version
    Info: Copyright (C) 1991-2005 Altera Corporation. All rights reserved.
    Info: Your use of Altera Corporation's design tools, logic functions 
    Info: and other software and tools, and its AMPP partner logic 
    Info: functions, and any output files any of the foregoing 
    Info: (including device programming or simulation files), and any 

    Info: associated documentation or information are expressly subject 
    Info: to the terms and conditions of the Altera Program License 

    Info: Subscription Agreement, Altera MegaCore Function License 
    Info: Agreement, or other applicable license agreement, including, 
    Info: without limitation, that your use is for the sole purpose of 
    Info: programming logic devices manufactured by Altera and sold by 
    Info: Altera or its authorized distributors.  Please refer to the 
    Info: applicable agreement for further details.
    Info: Processing started: Thu Nov 17 16:19:28 2005
Info: Command: quartus_sh -t DE2_Board_setup_quartus.tcl


Info: Evaluation of Tcl script DE2_Board_setup_quartus.tcl was successful
Info: Quartus II Shell was successful. 0 errors, 0 warnings
    Info: Processing ended: Thu Nov 17 16:19:28 2005
    Info: Elapsed time: 00:00:00

# 2005.11.17 16:19:29 (*) Completed generation for system: DE2_Board.
# 2005.11.17 16:19:29 (*) THE FOLLOWING SYSTEM ITEMS HAVE BEEN GENERATED:
  SOPC Builder database : C:/DE2/DE2_Board/system/DE2_Board.ptf 
  System HDL Model : C:/DE2/DE2_Board/system/DE2_Board.v 
  System Generation Script : C:/DE2/DE2_Board/system/DE2_Board_generation_script 

# 2005.11.17 16:19:29 (*) SUCCESS: SYSTEM GENERATION COMPLETED.


Press 'Exit' to exit.
